{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["办公椅1"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"办公椅1","index":0,"n_rows":6,"n_cols":5,"rows_kept":6,"merged":[[0,0,0,4],[6,0,6,4]],"flags":["formulas_cached_only"]}
["材质清单"]
[]
["序号","名称","采购数量","规格","材质"]
[1,"实木椅","20张","640*680*1060","基材：A级乌金木椅身，含水率低于15%，经过防虫、防腐等化学处理，密度700KG/m3以上，持久不变形，材质坚硬钢性强，承托力达300KG；2.油漆：采用优质环保漆，在恒温、恒湿高度防尘的面漆房喷涂面漆。经过最先进饱和漆工艺精心处理，从而保证台面平整无颗粒、气泡、渣点，颜色均匀；3.优质五金连接件。4、环保高密度、高弹性海绵。坐感更舒适柔软。软件包及缝纫外形泡满、圆滑一致、缝纫线迹均匀、嵌线圆滑挺直。5、一级牛皮面料，手感顺滑、柔软，纹理细腻真实，冬暖夏凉、工艺讲究，缝纫线条间隙大小均匀、流畅、转角平滑。"]
[2,"人体工学椅","20张","670*510*（1080-1200）","1、头枕、椅背、椅座均为进口过测试特网布；黑色塑胶框架；2、3D升降扶手，PU扶手面可前后、左右滑动；3、支架：背支架、背连接尾板、扶手支架均为铝件连接；85行程沉口4公分电镀汽杆；4、底盘：三级线控锁定同步倾仰底盘，带有倾仰调节功能，最大倾仰角度140度。 5、过BFM测试花瓣铝合金脚；65mmPU滑轮。\n"]
[3,"大班椅","35张","630*620*（1150-1200）","1、表面一级牛皮饰面，手感顺滑、柔软，纹理细腻真实，冬暖夏凉、工艺讲究，缝纫线条间隙大小均匀、流畅、转角平滑。\n2、骨架采用成型18MM曲木板。\n3、海绵：环保高密度、高弹性海绵。坐感更舒适柔软。软件包及缝纫外形泡满、圆滑一致、缝纫线迹均匀、嵌线圆滑挺直。\n4、脚架：电镀脚架配6寸黑色PU静音轮。\n5、协强气压泵，SGS认证3级85行程沉口4公分电镀汽杆，可承重300公斤压力。升降、倾仰，转动10万次以上无损。\n底盘：同步倾仰机构，可任意角度倾仰锁定。\n6、功能：可180度平躺。带脚踏。\n▲《办公椅》检测依据：QB/T2280-2016 外观要求 塑料件外观及软硬包件外观符合标准要求，力学性能要求：稳定性及座面冲击合格，扶手垂直向下静载荷和扶手水平静载荷，无断裂和豁裂、无明显变形，无松动，无失灵，合格。脚轮往复磨损。符合标准要求。底座静载荷7560N Imin,2次，底座的结构完整性应无破坏应无突然的明显的形变。符合标准要求。椅背往复耐久性，无断裂和豁裂现象无明显变形合格，跌落无松动，无失灵，无明显变形合格，阻然性要求：阻然1级通过香烟抗引燃特性试验合格。甲醛释放量≤0.02mg/m2h。TVOC≤0.03mg/m2.h。投标人须在投标文件中提供2022年1月1日至招标公告日前的副省级或以上质量检测部门出具的具有CMA资质成品抽样检验合格报告的复印件。"]