{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"images":2,"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":9,"n_cols":9,"rows_kept":9,"merged":[[0,0,0,8],[7,0,7,6],[8,1,8,8]]}
["中共深圳市委党校购置餐厅家具项目报价清单"]
["序号","名称","规格（W*D*H  mm)","详细技术参数","数量","单位","单价","合价","备注"]
[1,"书架轨道滑梯","11900W*3510H","1.高强度铝合金轨道、步梯，配耐磨抗氧化脚轮、带刹车功能，导轨轮。表面光滑平整，色泽均匀，喷塑层无漏喷、起泡、模糊、划痕或碰伤等缺陷，在接触人体或者收藏物品的部位无毛刺、刃口、棱角。承重力强，滑动阻力小。           2.整个梯子需要做内部加强处理，带折叠功能。根据现场实际情况定制。",1,"组"]
[3,"配餐柜","2113W*900D*800H","1、整体采用环保实木多层板烤漆工艺为基材，经过防潮、防虫、防腐化学处理。表面经过打磨、上底漆、烘干、抛光高温烤制而成，具有良好的耐高温、耐摩擦、自洁性等性能，表面平整、光滑，无纹路、桔皮现象承重能力强，\n2.采用优质五金配件，液压缓冲门铰开启、关闭灵活，优质五金锁具，铝合金拉手，经过防腐防锈处理。\n3、台面使用医用级人造大理石，耐磨耐刮耐高温，防渗透，防污渍。                                             4.所有的门板及外露侧面需要根据现场墙面同步做定制格栅。                                                                    5.根据柜体为方便以后搬动，需要配搬动工具一套",3,"组"]
[4,"餐桌","2400W*1200D*750H","1、桌面基材采用FAS级白蜡木实木台面，采用原木直拼板，非指接板\n2、钢脚：圆柱+圆盘脚，使用鞍钢一级冷轧钢板成型，壁厚不低于1.5mm，表面经静电粉末喷涂处理。                                                                               3.整张餐桌底部带支撑钢梁，防止台面变形，增加牢固度。",4,"张"]
[5,"折叠桌","1800W*400D","1.采用优质304不锈钢，厚度为1.5mm;\n2.不锈钢板经剪切，冲压，折弯，焊接，装配而成,焊接部分采用高标准熔接焊，表面平整光滑。   3.含多点固定支架。保证台面结实牢固",1,"张"]
[6,"搬家神器","参照图片","1.底轮可360度旋转\n2.承重400KG\n3.五件套",2,"套"]
[2]
["备\n注","1.以上报价应含税，运输、安装、搬卸、售后等所有费用；产品5年保修期，终生维护；  "]